**Adirondack Chair Assembly Instructions**

![A wooden chair in a grassy area

Description automatically generated with low confidence]()

Hardware Included

* 2- 20 x ¼” x 2 ½” carriage bolts
* 2- 20 x ¼” x 2 ¾” carriage bolts
* 4- ¼” flat washers
* 4- 20 x ¼” nuts
* 6- decorative bolt caps
* 8- #8 x 1 ¾” T20 screws
* 12- #8 x 2” T20 screws

Tools Needed for Assembly

* 7/16” wrench, 7/16” socket and rachet, or Adjustable wrench
* T20 screwdriver (included in hardware bag)
* Scissors or cutting tool, to remove packaging

A picture containing indoor

Description automatically generatedAssembly Instructions

1. Unpackage all the parts. Recommend pulling the back out first from the box. The front legs, arms and hardware bag will be inside the seat. The hardware bag will be in the box with the arms. Layout all the pieces in a clean work area.

A picture containing wooden, wood

Description automatically generatedA picture containing floor, wooden, seat, wood

Description automatically generated

2. Locate the front legs and the seat. Line up A1 on the right leg and A1 on the right side of the seat. Insert 1, 2 ½” carriage bolt through the center hole in the leg and pre screw in 2, 1 ¾” screws into the seat with 1/8” – ¼” length exposed on the outside to help line up with the screw holes in the leg. If aligned properly the front legs should have 4 screw holes at the top facing out for the arm to attach to. Once all 3 holes are lined up tighten done the screws with the included screwdriver and put on washer and nut onto the bolt. Tighten the bolt down and put a decorative cap on the end. Repeat this process for the other leg on the left side by lining up A2 and A2.

3. Loose up the nut B1 on the rear of the seat so the right rear leg moves freely. Repeat this for B2 on the other side for the left leg.

4. Locate the 2 arms. Pre screw in 4, 2” screws into the right arm at C1, with part of the screw sticking out the other side like in step 2. Line up the screws in C1 with the holes at C1 on the front right leg. Once lined up, screw the arm into the leg and tighten it done in a star pattern. Make sure the arm is flat against the leg. Repeat this process for the other side with C2 on the left front leg and C2 on the left arm.

A picture containing floor, seat, furniture

Description automatically generated

A picture containing person, indoor

Description automatically generated

5. Rotate the right rear leg up so D1 on the leg lines up with D1 on the right arm. The leg should be on the inside of the arm and at a slight angle inward. Look down the hole in rear of the arm to line up the bolt hole at the top of the rear leg. Once lined up insert 1, 2 ¾” carriage bolt through the arm into the leg. Put a washer and nut on bolt but **DO NOT TIGHTEN THE BOLT DOWN.** Leave both bolts on the rear leg loose. Repeat this process with D2 on the left leg and D2 on the left arm.

A picture containing indoor, wood

Description automatically generatedA picture containing ground, wooden, furniture, seat

Description automatically generated

A wooden bench in a room

Description automatically generated with low confidence

6. Locate the back. Pre screw 2, 2” screws into the lower back support at E1 and 2, screws at E2 like done in step 2 and 4. Rotate the back into place careful to not scratch up the wood with the screw Leave both screws loose with around ¼” of the screw not seated into the lower back support. ends. Rest the middle back on the rear of the arms. Line up the screw holes for the lower back support on both sides. Once lined up screw done connecting the lower back support with both sides of the seat. Leave both screws loose with around ¼” of the screw not seated into the lower back support.

A picture containing seat, sofa, feet

Description automatically generated

7. Make sure F1 on the back and F1 on the arm are lined up if they aren’t already. Then pre screw 2, 1 ¾” screws into the middle back support and line up the screw holes with screws like in step 2, 4, and 6. Once lined up screw in the screws but leave around ¼” of the screw not seated into the arm like in step 6. Repeat the same process for the left side with F2 leave the screws not fully seated. You may have to flex in the arm in to get the holes to line up.



A picture containing wooden, wood

Description automatically generated

8. Once all 8 screws on the back are seated into the holes tighten all the screws done at E1, E2, F1, and F2. Then tighten done the carriage bolts at B1, B2, D1, and D2. Then put the rest of the decorative bolt caps onto the remaining carriage bolts. Remove the sticker labels and enjoy your now assembled quality Redwood Adirondack chair. We recommend applying a desired finish once the labels are removed.

A picture containing chair, wooden, furniture, seat

Description automatically generatedA wooden chair in a room

Description automatically generated with medium confidence